**Plug-in free:**

|  |  |
| --- | --- |
| Supported Max. Resolution | <=3MP (I7 processor is required)**NOTE：**For the camera that the resolution is higher than 3MP, it may appear the phenomenon of previewing failed or black image. |
| Supported Browser | Firefox52+，Chrome45+，Safari 11+ |
| Supported Encoding Format | H.264, H.264+, H.265, H.265+ |

**Comparison Chart for Plug-in free and Plugin live view:**

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Function | Non-Plugin | With Plugin |
| Preview | Preview | Resolution<=3MP ((IE7 processor is required)Bitrate<=2M | √ |
| Audio | √ | √ |
| Capture | √ | √ |
| Digital Zoom | √ | √ |
| Window Division | √ | √ |
| Full-Screen | √ | √ |
| Record | √, Only Chrome | √ |
| Audio On | × | √ |
| Playback | Playback | × | √ |
| Download Video | × | √ |
| Picture | Picture | × | √ |
| Application | Application | √ | √ |
| Configuration | Export Device Parameters | √ | √ |
| Import Device Parameters | √ | √ |
| Upgrade | √(Only dav format file supported) | √ |
| Draw Area | √ | √ |
| Counting | Only support draw detection line. OSD display isn’t supported. | √ |
| Export Log | Support.txt format | √ |
| Local | × | √ |
| File Path Setting | Only file name can be displayed.It cannot show complete path. | √ |

**Involved Models:**

**IP camera**

All G1 platform cameras: DS-2CD2XX5, DS-2CD2XX3 V5.5.61\_180718 and above

All G1+M platform cameras: DS-2CD2XX6G1 V5.5.61\_180717 and above

All H3/H3+M platform cameras: DS-2CD5XXX, DS-2CD7XXX V5.5.50\_180309 and above

**NVR**

All I series NVR with V4.1.50\_180227 and above:

DS-76xxNI-I2, DS-76xxNI-I2/xP, DS-77xxNI-I4, DS-77xxNI-I4/xP, DS-96xxNI-I8, DS-96xxNI-I16

All Super I series with V4.1.61\_180818 and above:

DS-96000NI-I16, DS-96000NI-I16/H, DS-96000NI-I24, DS-96000NI-I24/H